MTT-part 
PN 16
DN 80/80
Cross-piece with four branches,
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on all sides,
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MTT-part

Pc 1   €/Pc .........   €/Item .........

MMB-part 
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on all sides,
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MMB-part

Pc 1   €/Pc .........   €/Item .........

Gate Valve 
for BAIO®plus System, tension proof,
PN 16
DN 80
Spigot end /Socket connection,
Body parts made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket and spigot end
for positive direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of plastic pipes,
socket designed for sealing ring to DIN 28 603,
with inserted GKS sealing ring for plastic pipes,
continuous pipe culvert,
boltless cover,
with inside screw,
wedge vulcanized all over with EPDM, with wedge drainage,
stem made of stainless steel with min. 13 % Cr,
maintenance-free stem seal,
(O-rings inserted in brass bushing)
Corrosion protection: 	inside and outside
			epoxy coating,
			blue, RAL 5005,
			according to GSK 

e.g. 	VAG BETA® 200 Gate Valve socket/spigot for plastic pipes
or similar

Options:	- with VAG VA telescopic equipment
	Adjustment range:	1.00 - 1.40 m
				1.20 - 1.80 m
				1.70 - 2.70 m
                  - with enclosed position indicator
	
Pc 1   €/Pc .........   €/Item .........

Gate Valve 
for BAIO®plus System, tension proof,
PN 16
DN 80
Socket connection on both sides,
Body past made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron pipes,
socket designed for sealing ring to DIN 28 603,
with inserted TYTON sealing rings for cast-iron pipes,
continuous pipe culvert,
boltless cover,
with inside screw,
wedge vulcanized all over with EPDM, with wedge drainage,
stem made of stainless steel with min. 13 % Cr,
maintenance-free stem seal,
(O-rings inserted in brass bushing)
Corrosion protection: 	inside and outside
			epoxy coating,
			blue, RAL 5005,
			according to GSK 

e.g. 	VAG BETA® 200 Gate Valve socket/socket for cast-iron pipes,
or similar

Options:	  - with VAG VA  telescopic equipment
	Adjustment range:	1.00 - 1.40 m
				1.20 - 1.80 m
				1.70 - 2.70 m
	- with fully enclosed position indicator
	
Pc 1   €/Pc .........   €/Item .........

Combination Gate Valve
for BAIO®plus System, resistant to tensile loads,
PN 16
DN 100(Spigot)/80(Branch)
Gate Valve branch DN 80…150
Fitting with same-size or reduced branch, 
resilient-seated BETA 200 Gate Valve in the lateral branch 
with socket connection to DIN 28603 and positive locking, 
tensile-load resistant internal lock for BAIO®plus System parts, 
and for the external locking of pipes, 
with inserted TYTON sealing ring for cast-iron pipes,
or with inserted GSK sealing ring for plastic pipes (PVC and PE)
Through-passage body with spigot end on either side and with locking cams 
for the tensile-load resistant connection with the VAG BAIO® BETA® socket Gate Valve 
or BAIO®plus socket fittings.
Body parts made of EN-JS 1030 (GGG-40) ductile cast iron, 
all components approved according to the KTW recommendations and DIN DVGW-W 270,
Application area: drinking water
Max. operating pressure: water 16 bar
Corrosion protection:	inside and outside
				epoxy coating
				RAL 5005 blue
				to GSK guidelines
=> For the connection to the pipe in the through-pipeline we recommend the use of the VAG BAIO®DVS double-socket locking part as divisible pipe coupling.

- Available connection sizes:	DN 100, branch DN 100;
  				DN 150, branch DN 80; 
				DN 150, branch DN 100; 
  				DN 150, branch DN 150.
 
e.g.	VAG BETA® 200 SMB Gate Valve
	- for cast-iron or plastic pipes
	- for the VAG BAIO®plus System

Optionally:	- with VAG VA telescopic installation equipment
		  Adjustment range:	1.00 - 1.40 m
					1.20 - 1.80 m
					1.70 - 2.70 m
		- with encapsulated position indicator

Quantity ........   Euro/Piece .........   Euro /Item .........

B-part 
PN 16
DN 100/80
with DN 80 socket on the side 
made of ductile iron EN-JS 1030 (GGG-40),
with double-function sockets and spigot end
for positive, direct interior interlocking 
with BAIO®plus System parts,
for exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®B-part

Pc 1   €/Pc .........   €/Item .........

EMS-part 
PN 16
DN 80
socket side allows sliding 
on the pipe end,
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on one side,
for positive, direct interior interlocking 
with BAIO®plus System parts,
with screwed socket on the other side to DIN 28 601, Part 2,
including rubber ring, sliding ring and threaded ring.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®EMS-part

Pc 1   €/Pc .........   €/Item .........

EN-part 
(Hydrant bend)
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
horizontal connection with double-function socket 
for positive, direct interior interlocking 
with BAIO®plus System parts and for 
exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603,
vertical connection designed as flange connection,
flange connection dimensions to DIN EN 1092,
can be supplied with three G 1½ outlets on the sides.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®EN-part

Selected version: with 2 thread outlet R1 1/2"

Pc 1   €/Pc .........   €/Item .........

EN-part 
(Hydrant bend)
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
horizontal connection with double-function socket 
for positive, direct interior interlocking 
with BAIO®plus System parts and for 
exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603,
vertical connection designed as flange connection,
flange connection dimensions to DIN EN 1092,
can be supplied with three G 1½ outlets on the sides.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®EN-part

Selected version: with 2 thread outlet

Pc 1   €/Pc .........   €/Item .........

EU-part 
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side,
for positive direct interior interlocking 
with BAIO® plus System parts and for
exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603,
with flange connection on the other side,
flange connection dimensions- to DIN EN 1092.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®EU-part

Pc 1   €/Pc .........   €/Item .........

F-part 
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with flange connection on one side,
flange connection dimensions to DIN EN 1092,
with spigot end on the other side,
for positive, direct interior interlocking 
with BAIO®plus System parts.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®F-part

Pc 1   €/Pc .........   €/Item .........

MMK-part 
PN 16
DN 80
11° / 22° / 30° / 45°-bend
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides
for positive, direct interior interlocking
with  BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MMK-part  ......° -bend

Selected version: 11 degree

Pc 1   €/Pc .........   €/Item .........

MMK-part 
PN 16
DN 80
11° / 22° / 30° / 45°-bend
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides
for positive, direct interior interlocking
with  BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MMK-part  ......° -bend

Selected version: 22 degree

Pc 1   €/Pc .........   €/Item .........

MMK-part 
PN 16
DN 80
11° / 22° / 30° / 45°-bend
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides
for positive, direct interior interlocking
with  BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MMK-part  ......° -bend

Selected version: 30 degree

Pc 1   €/Pc .........   €/Item .........

MMK-part 
PN 16
DN 80
11° / 22° / 30° / 45°-bend
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides
for positive, direct interior interlocking
with  BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MMK-part  ......° -bend

Selected version: 45 degree

Pc 1   €/Pc .........   €/Item .........

MMN-part 
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function sockets on both sides
for positive, direct interior interlocking 
with BAIO®plus system parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603
can be supplied with three G 1½ side outlets
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g.  VAG BAIO®MMN-part

Selected version: with 2 thread outlet

Pc 1   €/Pc .........   €/Item .........

MMN-part 
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function sockets on both sides
for positive, direct interior interlocking 
with BAIO®plus system parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603
can be supplied with three G 1½ side outlets
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g.  VAG BAIO®MMN-part

Selected version: without thread outlet

Pc 1   €/Pc .........   €/Item .........

MMQ-part 
90° quarter bend
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides 
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MMQ-part

Pc 1   €/Pc .........   €/Item .........

MSK-part 
45°-bend
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on one side,
with double-function socket on the other side,
for positive, direct interior locking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®MSK-part

Pc 1   €/Pc .........   €/Item .........

R-part 
PN 16
DN 100/80
Reducer for installation between spigot end and socket
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®R-part 

Pc 1   €/Pc .........   €/Item .........

RU-part 
PN 16
DN 80/125
Reducer for installation between socket and spigot end
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®RU-part 

Pc 1   €/Pc .........   €/Item .........

S-part 
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on both sides,
for positive, direct interior interlocking 
with BAIO®plus System parts.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®S-part

Selected version: 215mm

Pc 1   €/Pc .........   €/Item .........

S-part 
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on both sides,
for positive, direct interior interlocking 
with BAIO®plus System parts.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®S-part

Selected version: 500mm

Pc 1   €/Pc .........   €/Item .........

U-part 
PN 16
DN 80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides,
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
with or without side outlet female thread G2".
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g.  VAG BAIO®U-part

Selected version: with thread outlet

Pc 1   €/Pc .........   €/Item .........

SM-part 
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side
or double-function socket as a
transition to PE pipes having an
outer diameter of 125 or 180mm,
outer design allows the installation of a corresponding 
BAIO®plus-Stop tension guard,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603,
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®SM-part

Selected version: Long 150 mm

Pc 1   €/Pc .........   €/Item .........

SM-part 
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side
or double-function socket as a
transition to PE pipes having an
outer diameter of 125 or 180mm,
outer design allows the installation of a corresponding 
BAIO®plus-Stop tension guard,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603,
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®SM-part

Selected version: Long 200 mm

Pc 1   €/Pc .........   €/Item .........

SM-part 
PN 16
DN 80/80
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side
or double-function socket as a
transition to PE pipes having an
outer diameter of 125 or 180mm,
outer design allows the installation of a corresponding 
BAIO®plus-Stop tension guard,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603,
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®SM-part

Selected version: Long 300 mm

Pc 1   €/Pc .........   €/Item .........

TYTON EPDM sealing ring for cast-iron pipes
PN 16
DN 80
For water applications
suitable for pipes and form pieces
with sockets to DIN 28 603

e.g. VAG BAIO® TYTON sealing ring

Pc 12   €/Pc .........   €/Item .........

TYTON EPDM sealing ring for cast-iron pipes
PN 16
DN 100
For water applications
suitable for pipes and form pieces
with sockets to DIN 28 603

e.g. VAG BAIO® TYTON sealing ring

Pc 1   €/Pc .........   €/Item .........