MMB combination
Form piece with attached
Gate Valve for BAIO®plus System, tension proof,
PN 16
DN 80...200
Body parts made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket
for positive direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron or plastic pipes,
socket designed for sealing ring to DIN 28 603,
with inserted Tyton sealing ring for cast-iron pipes
or
with inserted GSK sealing ring for plastic pipes
continuous pipe culvert,
boltless cover,
with inside screw,
wedge vulcanized all over with EPDM, with wedge drainage,
EPDM wedge coating approved to KTW and W 270
stem made of stainless steel with min. 13 % Cr,
maintenance-free stem seal,
(O-rings inserted in bronze bushing)
Corrosion protection: 	inside and outside
			epoxy coating,
			blue, RAL 5005
			according to GSK 

e.g. 	VAG BETA® 200 MMB Combination for cast-iron or plastic pipes

Options:	- with hand wheel
	- with VAG VA telescopic equipment
	Adjustment range:	1.00 - 1.40 m
				1.20 - 1.80 m
				1.70 - 2.70 m
	   - with enclosed position indicator
	
Pc ........   Euro/Pc .........   Euro/Item .........