Underground hydrant PN 16
DN 80, with flange connection
similar to DIN 3221,
form A, with single shut-off, with safety interlock,
or
form AD, with double shut-off, in addition to automatic ball shut-off with safety interlock,
Body parts made of cast iron with spherical graphite,
with automatic drainage,
with pressure water protection
stem made of stainless steel with min. 13 % Cr,
maintenance-free stem seal,
(O-rings inserted in brass bushing),
all screws made of A2 stainless steel,
pressure pipe and connection pins made of stainless steel 1.4301, 
stem nut and valve seat bushing made of brass,
valve cone made of EN_JS 1050 (GGG-50), vulcanized all over,
with flange connection, 
including dirt and distortion protection,
Corrosion protection:	inside:  enamel
	          	outside: epoxy coating
		blue, RAL 5005, 
		according to GSK

Pipe cover: for 0.75 m, 1.00 m, 1.25 m or 1.50 m

DIN-DVGW registered

e.g. 	VAG BAIO® SUPRA 180V/280V Underground Hydrant, form A or AD 
version: Flange connection
or similar

Pc ........   Euro/Pc .........   Euro/Item .........