Welding end for PE-HD pipes
PN 16
DN 80 ... 200
designed as composite part,
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on one side, 
for positive, direct interior interlocking
with BAIO®plus system parts, 
with PE-HD pipe piece made of PE 100 on the other side,
firmly captivated with the cast-iron part, 
for welding with PE-HD pipes to make a welded socket joint
(welding factor 005...010 MFI) 

e.g. VAG BAIO®PEi welding end

Pc ........   Euro/Pc .........   Euro/Item .........