Combination Gate Valve
for BAIO®plus System, resistant to tensile loads,
PN 16
DN 100..150
Gate Valve branch DN 80…150
Fitting with same-size or reduced branch, 
resilient-seated BETA 200 Gate Valve in the lateral branch 
with socket connection to DIN 28603 and positive locking, 
tensile-load resistant internal lock for BAIO®plus System parts, 
and for the external locking of pipes, 
with inserted TYTON sealing ring for cast-iron pipes,
or with inserted GKS sealing ring for plastic pipes (PVC and PE)
Through-passage body with spigot end on either side and with locking cams 
for the tensile-load resistant connection with the VAG BAIO® BETA® socket Gate Valve 
or BAIO®plus socket fittings.
Body parts made of EN-JS 1030 (GGG-40) ductile cast iron, 
all components approved according to the KTW recommendations and DIN DVGW-W 270,
Application area: drinking water
Max. operating pressure: water 16 bar
Corrosion protection:	inside and outside
				epoxy coating
				RAL 5005 blue
				to GSK guidelines
=> For the connection to the pipe in the through-pipeline we recommend the use of the VAG BAIO®DVS double-socket locking part as divisible pipe coupling.

- Available connection sizes:	DN 100, branch DN 100;
  				DN 150, branch DN 80; 
				DN 150, branch DN 100; 
  				DN 150, branch DN 150.
 
e.g.	VAG BETA® 200 SMB Gate Valve
	- for cast-iron or plastic pipes
	- for the VAG BAIO®plus System

Optionally:	- with VAG VA telescopic installation equipment
		  Adjustment range:	1.00 – 1.40 m
					1.20 – 1.80 m
					1.70 – 2.70 m
		- with encapsulated position indicator

Pc ........   Euro/Piece .........   Euro /Item .........