Socket-end cap 
PN 16
DN 80 ... 200
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket,
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603,
with screwed-in malleable cast-iron plug.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			according to GSK

e.g. VAG BAIO®socket-end cap

Pc ........   Euro/Pc .........   Euro/Item .........