Spigot-end cap 
PN 16
DN 80 ... 300
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on one side,
for positive, direct interior interlocking 
with BAIO®plus System parts,
with screwed-in malleable cast-iron plug G 1 1/2“,
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®spigot-end cap

Pc ........   Euro /Pc .........   Euro /Item .........