U-part 
PN 16
DN 80 ... 200
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides,
for positive, direct interior interlocking 
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
with or without side outlet female thread G2”.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g.  VAG BAIO®U-part

Pc ........   Euro /Pc .........   Euro /Item .........