Pull-Lock for PVC pipes
PN 16
DN 80 ... 200
two-part design
consisting of:
- tension ring made of ductile iron EN-JS 1030 (GGG-40),
	Corrosion protection:	inside and outside
					epoxy coating
  					blue, RAL 5005
			
-	clamping ring made of grey plastic
	with corundum coating on the inside

e.g.	VAG BAIO®stop  Pull-Lock
		for PVC pipes

Pc ........      Euro/Pc .........     Euro/Item .........