Pull-Lock for cast-iron pipes
PN 16
DN 80 ... 200
two-part design
consisting of:
-  tension ring made of ductile iron EN-JS 1030 (GGG-40),
	Corrosion protection:	inside and outside
					epoxy coating
  					blue, RAL 5005
			according to GSK

-	clamping ring made of blue plastic
	equipped with stainless steel spikes on the inside

e.g.	VAG BAIO®stop Pull-Lock
		for cast-iron pipes
 
Pc ........   Euro /Pc .........   Euro/Item .........