Standpost Hydrant 
with spigot-end
with double sealing system
PN 16
DN 80…100
with safety locking system for internal parts
type AUD acc. to DIN 3222
knock-over design due to set of rupture nuts
due to a two-segment-loose-flange connection,
the upper pillar can be fixed during installation
steplessly (360°) in any position
with additional automatic float ball shut-off
body of ductile iron 
with automatic drainage and protection against loss of supply water
- two upper outlets, size B
- optional lower A-outlet
screws of stainless steel A2 
stem of stainless steel (min 13% Cr)
stem nut and main valve seat bush of brass
main valve cone of ductile iron, fully covered with rubber (EPDM),
with spigot end
Corrosion protection:	inside: true enamel
outside: primer enamel and acryl coating
colour fiery-red, RAL 3000
cover depth: 1,00m
DIN-DVGW approval

e.g. VAG NOVA 284 Standpost Hydrant 
version: Spigot-end

on request
-cover depth 1,00 m
-cover depth 1,25 m
-cover depth 1,50 m

Pc ..... Euro/pcs.....    Euro/item.....