VAG SUPRA 180V/280V
Underground Hydrant
PN 16 - DN 80

Product features
• Design acc. to DIN 3221, type A or AD
• Safety lock of the inner function unit
• Automatic draining and pressure water protection
• Maintenance-free stem seal with O-rings

Materials and corrosion protection
• Jacket and cover of ductile cast iron EN-JS 1050 (GGG-50)
• Valve cone of EN-JS 1050 (GGG-50), EPDM vulcanised
• Valve seat bushing of brass
• Inside true enamel, outside epoxy coating or
• inside and outside epoxy coating or
• body and valve seat epoxy coating
• Elastomers approved acc. to W 270
• Approved and registered by DVGW

Field of application
• Water distribution / water supply