Underground Hydrant
DN 80, PN 16
Type A
with a safety locking system for internal parts, 
with automatic drainage and protection against loss of supply water, 
body parts of ductile iron, 
stem of stainless steel, (min. 13% Cr.)
stem sealed with rubber 0-rings in brass bush, maintenance free 
screws and thrust pipe of stainless steel, 
stem nut and seat bush of brass,
main valve of ductile iron, fully covered with rubber (EPDM)
flange dimension to EN 1092, PN 16
Corrosion protection:	inside: true enamel, 
outside: epoxy coating blue, RAL 5005

		alternative: inside and outside epoxy coating

Cover depth: 0,75m

On request
- cover depth	1,00 m
- cover depth	1,25 m
- cover depth	1,50 m

e.g.  VAG SUPRA 180V Underground Hydrant 

Pcs. ..... Euro/pcs.....    Euro/item.....