VAG BAIO® plus System
VAG BAIO®BEV Automatic Air Valve
PN 16 - DN 80 / BAIO
Possible connections: flange or spigot

Product features
• High venting capacity
• Sturdy, stainless set for direct installation into the earth as
- standpost installation
- underground installation under a special street cap
• Protection jacket of stainless steel replaces the pit construction in its function

Materials
• Protection jacket and all inner parts of stainless steel
• VAG DUOJET® Automatic Air Valve: Body and cover of ductile iron EN-JS 1030 (GGG-40) - all inner parts of austenitic stainless steel
• Bonnet of corrosion resistant aluminium alloy

Field of application
• Substitute for pits