Automatic Air Valve
for potable water, with spigot-end
PN 16
DN 80 
for underground installation without pit construction
- venting into a street cap or
- venting above the ground level
consisting of:
- VAG DUOJET® Automatic Air Valve,
  compact single-chamber design with two venting functions,
  large orifice venting performance up to sonic speed,
  body parts made of ductile iron EN-JS 1030 (GGG-40),
  epoxy coating, inside parts and screws made of stainless steel A4,
  gaskets made of EPDM rubber,
- connection piece made of ductile iron EN-JS 1030 (GGG-40)
- epoxy coated, draining joint connection by screw fitting made of plastic material,
  connection to pipeline: BAIO®plus Joint DN 80,, 
 - protection jacket made of stainless steel, cap made of aluminium,
- further inside parts made of corrosion resistant steel or brass, 
Easy installation and dismantling of the valve,
automatic shut-off to the pipeline by rubber float ball.

example: VAG BAIO® BEV Automatic Air Valve
version: Spigot connection

optional: 
	- with special gasket for small operational pressures > 0,1 bar
	- with corresponding street cap type 3582
	- with rinsing set

Pc ........   Euro/Piece .........   Euro/Pos. .........