B-part 
PN 16
DN 80 ... 200
with DN 80 socket on the side 
made of ductile iron EN-JS 1030 (GGG-40),
with double-function sockets and spigot end
for positive, direct interior interlocking 
with BAIO®plus System parts,
for exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®B-part

Pc ........   Euro/Pc .........   Euro/Item .........