VAG BAIO®plus System
VAG BAIO®DVS Double-socket lock
PN 16 - DN 100...150

Product features
• For easy assembly (disassembly) of the BAIO®plus System
• For easy assembly (disassembly) of the pipeline
• Types:
-	divisible pipe coupling 
-	two-piece BAIO®U-part with externally lockable centre piece 
-	double-function socket on either side for positive internal locking with BAIO®plus System parts as well for external locking of cast-iron and plastic pipes.

Materials and corrosion protection
• ductile cast iron EN-JS 1030 (GGG-40) ductile cast iron 
• Inside and outside epoxy coating

Application area
• Water supply pipelines