EMS-part 
PN 16
DN 80 ... 300
socket side allows sliding 
on the pipe end,
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on one side,
for positive, direct interior interlocking 
with BAIO®plus System parts,
with screwed socket on the other side to DIN 28 601, Part 2,
including rubber ring, sliding ring and threaded ring.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®EMS-part

Pc ........   Euro/Pc .........   Euro/Item .........