EN-part 
(Hydrant bend)
PN 16
DN 80-100
made of ductile iron EN-JS 1030 (GGG-40),
horizontal connection with double-function socket 
for positive, direct interior interlocking 
with BAIO®plus System parts and for 
exterior interlocking of cast-iron and plastic pipes,
socket designed for sealing ring to DIN 28 603,
vertical connection designed as flange connection,
flange connection dimensions to DIN EN 1092,
can be supplied with three G 1½ outlets on the sides.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®EN-part

Pc ........   Euro/Pc .........   Euro/Item .........