F-part 
PN 16
DN 80 ... 200
made of ductile iron EN-JS 1030 (GGG-40),
with flange connection on one side,
flange connection dimensions to DIN EN 1092,
with spigot end on the other side,
for positive, direct interior interlocking 
with BAIO®plus System parts.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®F-part

Pc ........   Euro/Pc .........   Euro/Item.........