VAG BAIO®plus System
VAG BAIO®MMK-part

Product features
• Bend with bending angles of 11° / 22° / 30° / 45°
• With socket connections to DIN 28603on both sides
• For exterior interlocking with BAIO® tension protectors
• With double-function socket

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply