MMK-part 
PN 16
DN 80 ... 200
11° / 22° / 30° / 45°-bend
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on both sides
for positive, direct interior interlocking
with  BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®MMK-part  ......° -bend

Pc ........   Euro/Pc .........   Euro/Item .........