MMN-part 
PN 16
DN 80-100
made of ductile iron EN-JS 1030 (GGG-40),
with double-function sockets on both sides
for positive, direct interior interlocking 
with BAIO®plus system parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603
can be supplied with three G 1½ side outlets
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g.  VAG BAIO®MMN-part

Pc ........   Euro/Pc .........   Euro/Item.........