VAG BAIO®plus System
VAG BAIO®MMQ-part

Product feature
• Quarter bend (90°)
• With socket connection on both sides to DIN 28603
• For exterior interlocking with BAIO®plus tension protectors
• With double-function socket

Materials and corrosion protection
• Ductile iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply