VAG BAIO®plus System
VAG BAIO®MSK-part

Product feature
• 45°- bend
• Possible by means of interlocking several pipe cross-overs
• Spigot end with interlocking cams on one side
• Double-function socket for interior and exterior interlocking

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply