Weld-in end for PE-HD pipes
DN 80 (OD 90) ... 300 (OD 315)
with clamping ring for sockets, BAIO®plus System
Clamping ring made of EN-JS 1030 (GGG-40) ductile cast iron,
for the positive external locking between 
weld-in end and BAIO®plus socket, 
PE-HD pipe fitting made of PE 100,
for welding with PE-HD pipes (03-005 MFI), 
support sleeve made of stainless steel, 
pipe wall thickness to DIN 8074 SDR 11 (standard), 
Application area: drinking water 
Max. operating pressure: water 16 bar 

Corrosion protection:	inside and outside 
				epoxy coating,
				RAL 5005 blue
 
- Optionally, pipe wall thickness to DIN 8074 SDR 17
	- DN 80 (da 90)
                    - DN 100 (da 110)
	- DN 100 (da 125)                          
	- DN 125 (da 140)
	- DN 150 (da 160)
	- DN 150 (da 180)
	- DN 200 (da 200)
	- DN 200 (da 225)
	- DN 250 (da 250)
	- DN 250 (da 280)
	- DN 300 (da 315)
	- DN 300 (da 355)

e.g. VAG BAIO®PEa weld-in end

Pc ........   Euro/Pc .........   Euro/Item .........