VAG BAIO®plus System
VAG BETA® 200 Gate Valve
PN 16 - DN 80...300
Possible connections: Socket/Socket; Socket/Spigot or Flange/Spigot

Product features
• Resilient seated following EN 1171
• Screwless, pressure-sealed cover connection
• Inside stem screw
• Sealed socket connections on both sides for cast iron or plastic material pipes
• One side sealed socket connection, one side blunt end for internal locking
• One side flange connection, one side blunt end for internal locking

Materials and corrosion protection
• Body, wedge and cover of ductile iron EN-JS 1030 (GGG-40)
• Wedge vulcanized all over with EPDM
• Inside and outside epoxy coating acc. to GSK
• Elastomers approved acc. to KTW and W 270
• Approved and registered by DVGW

Field of application
• Water distribution, water supply
• Sockets and blunt ends designed for connections resistant to tensile strength with VAG BAIO®plus System equipment