S-part 
PN 16
DN 80 ... 200
made of ductile iron EN-JS 1030 (GGG-40),
with spigot end on both sides,
for positive, direct interior interlocking 
with BAIO®plus System parts.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®S-part

Pc ........   Euro /Pc .........   Euro /Item .........