Tension guard for cast-iron pipes
DN 80 ... 300
two-part design
consisting of:
- tension ring made of ductile iron EN-JS 1030 (GGG-40),

Corrosion protection: inside and outside
				 epoxy coating
  				 blue, RAL 5005
 		   according to GSK

-	Clamping ring made of elastomere, NIRO hooks vulcanised
	onto inside, separate clamping ring

e.g.	VAG BAIO®sit tension guard
		for PE-HD pipes

Pc ........   Euro/Pc .........   Euro /Item .........