SM-part 
PN 16
DN 80 ... 200
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side
or double-function socket as a
transition to PE pipes having an
outer diameter of 125 or 180mm,
outer design allows the installation of a corresponding 
BAIO®plus-Stop tension guard,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603,
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®SM-part

Pc ........   Euro/Pc .........   Euro/Item .........