VAG BAIO®plus System
VAG BETA® 200 SMB Gate Valve
PN 16 - DN 100...150
Branch DN 80…150

Product features
• Fitting with same-size or reduced branch
• VAG BETA® 200 Gate Valve in the lateral branch with socket connection to DIN 28603 
• With positive locking, tensile-load resistant internal lock for BAIO®plus System parts and for the external locking of pipes
• Resilient-seated in accordance with EN 1171
• Screwless, self-sealing cover
• Through-passage seat with spigot end on both sides and locking cams for tensile-load resistant connection to VAG BAIO®plus BETA® 200 Socket Gate Valves or BAIO®plus socket fittings

Materials and corrosion protection
• Body made of EN-JS 1030 (GGG-40) ductile cast iron 
• Inside and outside epoxy coating according to the GSK guidelines
• Elastomers approved according to KTW and W270
• DVGW approved

Application area
• Water supply pipelines
• Tensile-load resistant connection with VAG BAIO®plus System parts