VAG BAIO® plus System
Soft sealing, one side flange connection, one
side blunt end with locking cams
PN 16 – DN 80...300

Product features
• Soft sealing following EN 1171
• Inside stem screw
• Screwless, pressure-sealed cover connection
• One side flange connection acc. to EN 1092-2 PN 10/16, one side blunt end with locking cams for connections resistant to tensile strength with VAG BAIO® plus system equipment

Materials and corrosion protection
• Body, wedge and cover of ductile cast iron EN-JS 1030 (GGG-40)
• Wedge all around EPDM vulcanised
• Inside and outside epoxy coating acc. to GSK
• Elastomers approved acc. to KTW and W 270
• Approved and registered by DVGW

Field of application
• Water supply lines
• Blunt ends designed for connections resistant to tensile strength with VAG-BAIO® plus System equipment