VAG BEV Automatic Air Valve
PN 16 - DN 80

Product features
• High venting capacity
• Sturdy, stainless set for direct installation into the earth as
- standpost installation
- underground installation under a special street cap
• Protection jacket of stainless steel replaces the pit construction in its function

Materials
• Protection jacket and all inner parts of stainless steel
• DUOJET® body and cover of ductile iron EN-JS 1030 (GGG-40)
- all inner parts of austenitic stainless steel
• Bonnet of corrosion resistant aluminium alloy

Field of application
• Substitute for pits