Automatic Single Chamber Air Valve, 
PN 16 -  DN 25
for water, with inside thread in acc. 
with DIN ISO 228-1, G ¾ / G 1 / G 1 ¼ 
single chamber design,
body and bonnet of ductile iron, EN-JS 1030 (GGG 40)
float of plastic,
socket threat G1" to DIN ISO 288-1,
gasket of rubber (NBR),
Corrosion protection: 	inside and outside
epoxy coating,
blue, RAL 5005

e.g.  VAG Single Chamber Air Valve, BEV-E

on request:	- female thread G¾" or G 1¼"
		- pressure rate PN 25
- with integrated cock for shut/off

pcs.....    	Euro/pcs.....    		Euro/item.....