Underground hydrant PN 10
DN 50
Jacket pipe, cover, claw etc. made of cast iron EN-JL 1040 (GG-25),
with automatic drainage,
with pressure water protection,
stem made of stainless steel with min. 13 % Cr,
maintenance-free stem seal,
valve cone made of EN-JL 1040 (GG-25), with NBR rubber coating,
pressure pipe made of stainless steel,
stem nut made of EN-JS 1050 (GGG-50),
screws and nuts made of A2 stainless steel,
flange connection dimensions to DIN 2501-1,
Corrosion protection: 	inside and outside
		epoxy coating, 
		blue, RAL 5005

Pipe cover: for 1.00 m, 1.25 m or 1.50 m

e.g. VAG underground hydrant DN 50 
or equivalent

Options:		Designed as car wash hydrant
		with 2 valve outlets that can be shut off 
	  	and with Storz 32 fixed couplings

Pc ........   Euro/Pc .........   Euro/Item .........