GKS cast-iron plastic sealing ring
for PVC and PE-HD pipes
PN 16
DN 80 ... 200
For water applications
suitable for pipes and form pieces
with sockets to DIN 28 603

e.g. VAG BAIO® GKS sealing ring

Pc ........   €/Pc .........   €/Item .........