VAG BAIO®plus System
VAG BAIO®U-part

Product features
• Connection form piece with socket on both sides
• Sockets designed as double-function sockets for interior and exterior interlocking; equipped with a stop to prevent the pipe being pushed through

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply