VAG BAIO®plus System	
VAG BAIO®B-part

Product feature
• Form part for branches, mainly as a connection for hydrants directly mounted to the pipeline
• In bore direction with socket - spigot connection DN 100, 150 and 200
• With DN 80 spigot connection in the branch
• Socket designed as double-function socket for interior and exterior interlock
• Spigot end with interlocking cams

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply