VAG BAIO®plus System
VAG BAIO®EMS-part

Product feature
• For repair / replacement or later extension of pipework parts
• With spigot connection with interlocking cams on one side for interior interlocking
• With UNION screw socket on the other side for connection to cast iron pipes; with green UNION sealing ring also   suitable for use with plastic pipes
• Can be shifted on the spigot end of the pipe
• Tension protection available on request

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply