VAG BAIO®plus System
VAG BAIO®F-part

Product feature
• Flanged on the one side
• On the other side spigot

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply