VAG BAIO®plus System
VAG BAIO®MMB-part

Product features
• Form piece for branches with 3 socket connections
• Sockets designed as double-function sockets for interior and exterior interlocking

Materials and corrosion protection
• Ductile cast iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply