VAG BAIO®plus System
VAG BAIO®X-part Socket end cap

Product features
• To close the spigot end of cast-iron, PVC and PE-HD pipes (e.g. during pressure tests)
• Longitudinal non-positive lock by means of the BAIO®plus tension protectors suitable for the respective pipe materials used
• With test and vent plug

Materials and corrosion protection
• Ductile iron EN - JS 1030 (GGG-40)
• Inside and outside epoxy coating

Field of application
• Water distribution / water supply