VAG BAIO®plus
weld-on ends/ form parts BAIO® PEi

Product features
• Positive locking interior interlock between weld-in end and BAIO®plus socket
• Weld-in end made of PE 100 with integrated interlocking ring and screwed on protection collar with twist protection
• Sealing of weld-in ends by commercially available TYTON rings
• Detachable connections

Materials and corrosion protection
• Weld-in end made of PE 100
• Locking ring made of ductile iron EN - JS 1030 (GGG-40)
• Protection sleeve made of EPDM

Field of application
• Water distribution / water supply