VAG BAIO®plus System
BAIO®Pea Weld-in End
DN 80…300

Product features
• For positive external locking between weld-in end and 
  BAIO®plus socket
• Weld-in end for PE-HD pipes with clamping ring for sockets

Materials and corrosion protection
• Weld-in end made of PE 100
• Locking ring made of EN-JS 1030 (GGG-40) ductile cast iron 
• Inside and outside epoxy coating
• Supporting sleeve made of stainless steel

Application area
• Water supply pipelines