RU-part 
PN 16
DN 125>80...150>100
Reducer for installation between socket and spigot end
made of ductile iron EN-JS 1030 (GGG-40),
with double-function socket on one side,
with spigot end on the other side,
for positive, direct interior interlocking
with BAIO®plus System parts and for
exterior interlocking of cast-iron and plastic pipes.
Socket designed for sealing ring to DIN 28 603.
Corrosion protection:	inside and outside
			epoxy coating
			blue, RAL 5005
			
e.g. VAG BAIO®RU-part 

Pc ........   Euro/Pc .........   Euro/Item .........