VAG BEV-E Air Venting Valve
PN 16/25 - DN 25 / female thread
G 3/4", G 1", G 1¼"

Product features
• Single chamber air valve, directly operated by the flow medium
• Venting small amounts of air in domestic water supply pipelines during operation
• To be screwed onto the pipeline

Materials and corrosion protection
• Body lower and upper part of ductile iron EN-JS 1030 (GGG-40)
• Floater of plastic material
• All other inner parts of bronze
• Inside and outside epoxy coating

Field of application
• Domestic water supply systems